FY 2014 NFSN WORK PLAN GUIDANCE 
Sampling at sites in the National Fixed Site Network
September 2013


FY2014 will be the second year under the NAWQA Cycle 3 design.  Water-quality sampling at sites in the National fixed Site Network (NFSN) will continue under the same design used during FY 2013. The Cycle 3 design includes the following features:

[bookmark: _GoBack]Water-quality samples collected at the National Fixed Site Network (NFSN) sites will include the following:
	Field measurements (air temperature, water temperature, pH, dissolved oxygen, 
		specific conductance, and alkalinity)
	Suspended Sediment - concentration and sand/fine break 
	Nutrients and Carbon (SH2430 or SH2431 or SH2432)
	Major Ions (SH998 or SH1201)
	Pesticides (SH2437) Note: pesticide samples should not be collected at the 			reference sites.
	
Ecological samples will be collected at all 39 NFSN sites categorized as urban (10 sites), agricultural (10 sites), or reference (19 sites).  Samples collected will include the following:
	Invertebrate -RTH (LC2172)
	Algae-RTH 
	Chlorophyll a and biomass (SH1632)
	Fish
	Habitat
  
There are currently 100 sites in the Cycle 3 NFSN. Water-quality samples will continue to be collected every year at all sites. These sites include those from the National Water Quality Assessment (NAWQA), National Stream Quality Accounting Network (NASQAN), and National Monitoring Network (NMN) programs. Separate guidance documents and surface-water sampling plans (SWPLANs) are no longer issued for each network. The three networks will follow the same protocols for sample collection and processing. NAWQA large river sites, as much as possible, were selected for inclusion in the Cycle 3 NFSN with the intent of complementing those already in the NASQAN and NMN networks. Data analysis and interpretation will be integrated so that products reflect findings of the NFSN rather than separate programs. Ecological samples will be collected every year at the urban, agricultural, and reference sites. No ecological samples will be collected at the large river sites. Please refer to the FY 2014 NFSN SWPLAN for site information such as site type and network category.
The following samples will be collected at select large-river sites (most are NASQAN or NMN sites): 
	DOC fractionation (George Aiken) 
	DNA (Byron Crump)
	Isotopes (Ty Coplen)
	Mercury (George Aiken)
	Tritium (Megan Young)

Please refer to Attachments 8, 9, and 10 in this document for sampling and processing guidance for DOC fractionation, DNA, and isotope sampling, respectively. Information on mercury sampling will be sent as a separate document. Please refer to the FY 2014.NFSN.SWPLAN.xlsx for sample requirements at each NASQAN and NMN site.   

Seasonally-weighted fixed interval sampling will be used (no storm chasing).  That is, fixed interval sampling is used but the intervals between samples vary given the time of year. Please contact Dave Reutter if a sampling trip must be rescheduled. The number of water samples collected per year at each site varies based on size, location, and chemical use in the basin.   FY2014.NFSN.design.xlsx (worksheet ‘Sampling Frequency’) gives the number of samples per month for each site.  

Ecological sampling will include annual sampling for Invertebrates (RTH only), Algae (RTH and chlorophyll/biomass), Fish, and Habitat. There will be no changes in the ecological sampling protocols from those used in Cycle 2.  Habitat data collection activities have been reduced such that all ecological sampling can be collected in a shortened time period. New field sheets have been developed to reflect these reductions. Please contact Amanda Bell if you have questions.   

FY 2014 targets for water-quality sampling have been developed based on prior years cost to sample the sites. Budget targets for ecological sampling in FY 2014 are based on Cycle 2 assumptions, with sampling responsibilities assigned to the SC that was responsible for ecological data collection at the site in Cycle 2. Targets in future years will likely be lower to reflect a reduced overall sampling effort.  


Cycle 3 SWPLAN

NFSN Chemical Sampling
Review the FY 2014 information – Please review the number of planned environmental samples, along with the requirements for QC samples (blanks, replicates, and spikes), shown for each site in the Cycle 3 NFSN SWPLAN.  Finally, review the streamflow gaging and continuous monitoring information (columns J through N).  

NFSN Ecological Sampling
Review the FY 2014 information for all sample types and verify all information for the site(s) to be sampled by your SC.  Please contact Amanda Bell for clarification if you have any questions about planned sampling activities. 
Ecological sampling will be conducted within the defined 6-week Index Periods as indicated in the SWPLAN spreadsheet; these Index Periods remain the same for FY 2014 as in previous years.  Any anticipated departures from sampling during the Index Period should be discussed in advance with Amanda Bell.

Annual review of ecological data is the responsibility of the Science Center (SC) that was responsible for collecting the samples.  Refer to Attachment 5 for details.

Fish Quality Assurance (QA) Plans must be updated annually by Science Centers responsible for collecting NAWQA fish community samples.  Enter “Yes” or “No” in column Y to indicate whether your Fish QA Plan has been reviewed/updated for the current fiscal year and submitted to Mike Meador (mrmeador@usgs.gov); an entry should be made for each site for years when fish are to be (or were) sampled. Refer to Attachment 6 for details.  


Preparing the NFSN budget for your SC

A set of spreadsheets in the file FY 2014.NFSN.Budget.WPG.xlsx is available to help you fill in your budget template.  The worksheet “SW sites” gives total site costs that were used to estimate sampling costs for the sites.  The FY 2014 Eco site net costs” contain net costs by category (field and office labor, vehicles, supplies, etc.) for the ecology sampling costs.  Estimated costs are summarized by SC in the “FY 2014 sampling by SC” worksheet.  All costs are in FY 2014 dollars.  

Funds for depreciation/replacement of capital equipment have been included in the water chemistry cost targets. These funds are to replace field equipment (including vehicles) when needed.  It is expected that most of these funds will be put into a working capital fund so that they are available when needed to replace expensive items.  While these funds alone will probably not be sufficient to replace vehicles, they should be sufficient to cover the NAWQA portion of vehicle purchases.  These items are too expensive to be covered by NAWQA in any given year and inclusion of funds in the targets to be placed in a working capital fund is an attempt to amortize the cost of these items to the program.  Because of funding limitations, there can be no line item allocations of NAWQA funds to cover purchases of vehicles.
. 
Management costs associated with sampling have been included in the water quality and ecology sampling budget targets.  Management costs should be included in the corresponding subtask column (e.g. “Surface Water QW with/without Streamgaging Site #1”, “Surface Water Eco Site #1“) of the “FY 2014.SC.BudgetTemplate” spreadsheet.  Do not include these management costs elsewhere.  
  
In calculating ecology sampling budget targets, no costs for contracts or equipment have been included; this is because such costs are expected to be highly variable among SCs.  Costs for contracts and equipment should be itemized in the budget requests and are considered as separate from the ecology targets.  Training costs associated with the Ecological Field Methods course, if offered, and for electrofishing (initial certification or refresher training) will be covered by headquarters funds; training needs for these courses should be indicated in the training spreadsheet (see below).  Annotate any requests for contracts, equipment, or training (other than field methods or electrofishing) in the comment rows in the Budget Template.

Please remember to complete the information requested in the training spreadsheet in the Budget Template. Additional columns are included for ecological training needs.  Please enter “X” (crew member) or “CL” (crew leader) for ecological sampling; if different individuals are typically responsible for different ecological components, adding that information as “CL-Inv”, “CL-Alg”, or “CL-Hab” would be helpful.  Because of the separate training requirements for electrofishing (to be in compliance with Bureau safety policy), a separate column is provided to indicate crew member (“X”) or Electrofishing Crew leader (“ECL”) for electrofishing.  Although it is expected that crew composition may change, this information will help establish the need, and priorities, for training.  Current information on past training for ecological field methods (Ecological Field Methods Course, or previous “TAMS” training), and electrofishing is provided; please update this information and indicate priority candidates for training.  Be aware of the Bureau safety policy requirement for electrofishing crew leaders to take “Principles and Techniques of Electrofishing” (National Conservation Training Center), and at 5-year intervals a refresher course (minimum 2 days) that has been approved by the Regional Safety Manager.

Guidelines for NFSN chemical sampling procedures for FY 2014 are attached (Attachments 1-4). Further details will be provided later this summer. SC personnel are responsible for data review, rerun requests, and timely responses to contamination problems and other data issues. 

Please refer any specific questions about the SWPLAN to Dave Reutter (614-430-7732, dreutter@usgs.gov).  General questions about the budget target, FY 2014 budget guidance, or the NFSN design should be addressed to Charlie Crawford (317-600-2776, cgcrawfo@usgs.gov).  Questions concerning index periods or other technical questions related to implementing ecological sampling protocols should be directed to Amanda Bell (608-821-3882, ahbell@usgs.gov). Technical questions related to implementing water-quality sampling protocols should be directed to Dave Reutter or Charlie Crawford.
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Attachment 1. FY 2014 NFSN Operations


Laboratory Information

Account Number
Please refer to the NFSN SWPLAN to verify the program your site is listed under (Cycle 3 Network Category). All ecological work will be funded by NAWQA.

An account number established by each SC will be required on the NWQL Analytical Service Request (ASR) for all samples collected from the NAWQA, NASQAN, and NMN sites. 
Note:  This is a change to the accounting system that has been used in previous years by the NASQAN and NMN programs.

Proposal Number
For NAWQA, NASQAN, and NMN sample submittals, enter the FY14 Proposal number as CL14NAW (and 2 letter state abbreviation). 

Program/Project Code
Under Program/Project Code, enter one of the following codes:
SWMSA 		NAWQA Surface Water Monitoring & Status Assessment 
NASQAN 		National Stream-Accounting Network	
NMN			National Monitoring Network 

These codes are needed for accounting and data review activities. 

Laboratory Schedules
Laboratory schedules for analysis of NFSN samples at the NWQL are listed below. There are several choices for routine analyses of both nutrient and major ions, depending upon expected concentrations. The appropriate schedule for each station is to be selected to avoid nondetects. Questions about this issue should be addressed to the NFSN Sampling Coordinator.

Schedules and Lab Codes
Nutrients – use either Schedule 2430, 2431, or 2432. The differences in lab schedules are as followed:
2430 Nutrients, particulate carbon, nitrogen, organic carbon, inorganic carbon 
(Total Phosphorus Reporting Level = 0.02 mg/L; nitrite+nitrate Reporting Level = 0.04 mg/L)

2431 Nutrients (low-level total phosphorus), particulate carbon, nitrogen, organic carbon, and inorganic carbon
(Total Phosphorus RL = 0.004 mg/L; nitrite+nitrate RL = 0.04 mg/L)

2432 Nutrients (low-level total phosphorus and nitrite+nitrate), particulate carbon, nitrogen, organic carbon, and inorganic carbon
(Total Phosphorus RL = 0.004 mg/L; nitrite+nitrate RL = 0.01 mg/L)

Major ions – use either Schedule 998 or Schedule 1201.  The differences in lab schedules are as followed:
Schedule 998 -- Major ions and miscellaneous trace elements (conductance < 2000)
Schedule 1201-- Major ions and miscellaneous trace elements (conductance > 2000)

2437 Pesticides in filtered water 

Updated information from the NWQL on sample requirements for these schedules can be obtained from the NWQL web page (http://nwql.cr.usgs.gov/usgs/catalog/index.cfm).

Suspended- Sediment 
Laboratories
WSCs may now use the approved USGS sediment lab of their choosing that is capable of doing both suspended sediment concentration and the sand/fine split. If more than one bottle is needed to collect a sample, please request the sediment lab to composite the sediment bottles before analysis (only one sediment bottle analyzed). Samples should be analyzed for concentration and sand-fine break.

Tritium, isotope, DOC fractionation, and DNA samples
Tritium, Isotope, DOC fractionation, and DNA samples will be collected at select sites. Please refer to FY2014.NFSN.SWPLAN.xlsx for site information. Please refer Attachments 8 and 9 for sampling protocols for DOC fractionation and DNA samples, respectively. 

Quality-Control
The specific types of QC samples to be collected at each NFSN station are described in the SWPLAN provided by the NFSN Coordinator. Guidelines for collection, processing, and coding of QC samples are provided in Attachments 2 and 3. Please carefully follow the coding instructions for all QC samples. Consistency across the network is necessary for efficient analysis of the QC data. Standard SC quality-assurance procedures (for example, periodic review of field operations and data quality by the SC Water Quality Specialist) should be done for NFSN operations.



Attachment 2.  NFSN Water-Quality Sampling Protocols

[bookmark: HDR0]Introduction
This document provides an overview of standard methods for collecting and processing water-column samples for the NFSN program. The methods are intended to provide water-quality data oriented to meet the specific goals of NFSN, and conform to established methods of the U.S. Geological Survey as described in detail in the National Field Manual for the Collection of Water-Quality Data (http://water.usgs.gov/owq/FieldManual/index.html). Additional information on the rationale for and complete description of these sampling and processing procedures are also contained in Edwards and Glysson (1999), as well as selected Technical Memoranda issued by the Office of Surface Water (Technical Memorandum 94.05; http://water.usgs.gov/admin/memo/SW/sw94.05.html) and Office of Water Quality [Technical Memorandum 97.06 ] (http://water.usgs.gov/admin/memo/QW/qw97.06.html).
Constituents routinely measured by the NFSN program include field parameters (water temperature, air temperature, specific conductance, dissolved oxygen, and pH), suspended sediment, major ions (including alkalinity), nutrients, dissolved/particulate carbon, and pesticides. 
Specific information regarding the analytical method for particulate carbon/nitrogen is available as follows: OWQ Tech Memo 2000.05 (http://water.usgs.gov/admin/memo/QW/qw00.05.html) and OWQ Tech Memo 2000.08 (http://water.usgs.gov/admin/memo/QW/qw00.08.html).
[bookmark: HDR1]Sampling equipment
To the greatest extent possible, isokinetic sampling techniques that provide samples representative of stream conditions are required by the NFSN program.   In 2002, the Office of Water Quality, in concurrence with the Office of Surface Water, recommended that the US D-77 rigid-bottle and bag samplers and the frame-type bag sampler be phased out for collection of water-quality and sediment samples. The US DH-81,US DH-2, US DH-95, US D-95, US D-96, and US D-99 isokinetic samplers have been approved by the Interagency Technical Committee of the Subcommittee on Sedimentation and provide the field with a well-tested and documented set of samplers that work in most sampling conditions. Accordingly, the D-77 rigid-bottle and bag samplers should have been replaced with the newer samplers. Please contact the NFSN Coordinator (Charlie Crawford) if one of the discontinued samplers still is being used.
The decision on which sampler to use is based upon the hydrologic conditions in the stream, the limits of the samplers, and informed judgment in the field, all of which are essential for collecting a representative sample. Further information is available for the samplers at: 
http://pubs.usgs.gov/of/2005/1087/book_2.html

For information on USGS guidelines for equipment selection, consult Chapter 2 in the National Field Manual and USGS Open-File Report 2005-1087 – A Guide to the Proper Selection and Use of Federally-Approved Sediment and Water-Quality Samplers.

Water-quality samplers
A brief overview of the more commonly-used samplers is provided below.
1. DH-2 (and DH-2a)
· must be coated with Plasti-Dip to prevent trace-element contamination---if plastic coating becomes scratched, reapply Plasti-Dip (spray plastic paint, available locally or online- www.usplastic.com is a source)
· collects a maximum of 1 L sample per vertical
· approved for flow velocities between 2 to 6 ft/s
· nozzle sizes are 3/16, 1/4, and 5/16 inch and give the sampler the capability to sample to depths of 37, 20, and 13 feet, respectively
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon.
· Use disposable poly bags for all samples except pesticides
· Use disposable Teflon bags for the collection of pesticides
· Follow the guidelines for bag sampler intake efficiency tests and operational velocities as described in OWQ TM 13.02.
1. Perform field tests of bag-sampler intake efficiency before each set of samples is collected during site visits; 
2. Store the required data (five parameters) from these tests in the National Water Information System (NWIS) with associated environmental samples; and 
3. Incorporate the revised, temperature-indexed minimum stream velocities (Table 1) for bag samplers into data-collection practices where suspended sediment may include a significant percentage of material larger than silt size (≥0.062 mm). 
2. DH-81
· suspended from a rod--used for wadeable streams
· uses standard D-77 cap and accessories, 1-L bottle
· collects a maximum of  800 mL sample per vertical
· approved for flow velocities between 1.5 and 7.6 ft/s
·  nozzle sizes are 3/16, 1/4, and 5/16 inch and give the sampler the capability to sample to depths up to 12 ft
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon.  Sediment samples can be collected in plastic bottles.
3. D-95
· must be coated with Plasti-Dip to prevent trace-element contamination---if plastic coating becomes scratched, reapply Plasti-Dip (spray plastic paint, available locally or online- www.usplastic.com is a source)
· collects a maximum of 1 L sample per vertical  (recommended 800 mL sample per vertical)
· approved for flow velocities between 1.5 to 7.5 ft/s
· nozzle sizes are 3/16, 1/4, and 5/16 inch 
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon. Sediment samples can be collected in plastic bottles.
4. DH-95
· must be coated with Plasti-Dip to prevent trace-element contamination---if plastic coating becomes scratched, reapply Plasti-Dip (spray plastic paint, available locally or online- www.usplastic.com is a source)
· collects a maximum of 1 L sample per vertical (recommended 800 mL sample per vertical)
· approved for flow velocities between 1.7 to 7.4 ft/s
· nozzle sizes are 3/16, 1/4, and 5/16 inch 
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon. Sediment samples can be collected in plastic bottles.
5. D-96
· must be coated with Plasti-Dip to prevent trace-element contamination---if plastic coating becomes scratched, reapply Plasti-Dip (spray plastic paint, available locally or online- www.usplastic.com is a source)
· collects a maximum of nearly 3 L sample per vertical
· approved for flow velocities between 2 to 12.5 ft/s
· nozzle sizes are 3/16, 1/4, and 5/16 inch and give the sampler the capability to sample to depths of 110, 60, and 39 feet respectively
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon.
· Use disposable poly bags for all samples except pesticides
· Use disposable Teflon bags for the collection of pesticides
· Follow the guidelines for bag sampler intake efficiency tests and operational velocities as described in OWQ TM 13.02.
1. Perform field tests of bag-sampler intake efficiency before each set of samples is collected during site visits; 
2. Store the required data (five parameters) from these tests in the National Water Information System (NWIS) with associated environmental samples; and 
3. Incorporate the revised, temperature-indexed minimum stream velocities (Table 1) for bag samplers into data-collection practices where suspended sediment may include a significant percentage of material larger than silt size (≥0.062 mm). 
6. D-96- A1
· must be coated with Plasti-Dip to prevent trace-element contamination---if plastic coating becomes scratched, reapply Plasti-Dip (spray plastic paint, available locally or online- www.usplastic.com is a source)
· collects a maximum of nearly 3 L sample per vertical
· approved for flow velocities between 2 to 6 ft/s
· nozzle sizes are 3/16, 1/4, and 5/16 inch and give the sampler the capability to sample to depths of 110, 60, and 39 feet respectively
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon.
· Use disposable poly bags for all samples except pesticides
· Use disposable Teflon bags for the collection of pesticides
· Follow the guidelines for bag sampler intake efficiency tests and operational velocities as described in OWQ TM 13.02.
1. Perform field tests of bag-sampler intake efficiency before each set of samples is collected during site visits; 
2. Store the required data (five parameters) from these tests in the National Water Information System (NWIS) with associated environmental samples; and 
3. Incorporate the revised, temperature-indexed minimum stream velocities (Table 1) for bag samplers into data-collection practices where suspended sediment may include a significant percentage of material larger than silt size (≥0.062 mm). 
7. D-99
· must be coated with Plasti-Dip to prevent trace-element contamination---if plastic coating becomes scratched, reapply Plasti-Dip (spray plastic paint, available locally or online- www.usplastic.com is a source)
· collects a maximum of nearly 6 L sample per vertical
· approved for flow velocities between 3 to 15 ft/s
· nozzle sizes are 3/16, 1/4, and 5/16 inch and give the sampler the capability to sample to depths of 220, 120, and 78 feet respectively
· Teflon® is required for all components that are in contact with the water sample for organic analysis—nozzle holder, and nozzles. Plastic components are adequate for inorganics and carbon.
· Use disposable poly bags for all samples except pesticides
· Use disposable Teflon bags for the collection of pesticides
· Follow the guidelines for bag sampler intake efficiency tests and operational velocities as described in OWQ TM 13.02.
1. Perform field tests of bag-sampler intake efficiency before each set of samples is collected during site visits; 
2. Store the required data (five parameters) from these tests in the National Water Information System (NWIS) with associated environmental samples; and 
3. Incorporate the revised, temperature-indexed minimum stream velocities (Table 1) for bag samplers into data-collection practices where suspended sediment may include a significant percentage of material larger than silt size (≥0.062 mm). 
8. Support equipment
· when using metal support equipment, such as cranes and reels, or sampling from bridges or cable cars, always use the clean hands/dirty hands technique--GREAT CARE IS NEEDED TO AVOID CONTAMINATING THESE SAMPLES.
· to prevent contamination during sample processing, field vehicles will ideally be dedicated to water-quality work
· when a dedicated WQ vehicle is not available, the processing area in the vehicle must be free of contaminants including metallic objects, dirt, and oil residue
· separate storage areas for the sampling equipment must be available
· prepare areas separately for processing inorganic and organic samples; if necessary, cover metal cabinets and shelves with plastic sheeting before processing the inorganic samples and cover the counter space with aluminum foil before processing organic compounds
· processing and preservation chambers must be used for processing inorganic constituents; use portable chambers for multi-use vehicles
· field equipment blanks must be collected regularly 

9. Suspended sediment

	Suspended-sediment samples should be collected separate from the water-chemistry samples. The 	suspended sediment sample should no longer come from the churn or cone splitter.

	When using the EDI method, an individual bottle of equal sample volume should be collected at 	each vertical. Please request that the bottles be combined at the sediment lab for a single sediment 	analysis.  The EWI sampling method does not require an individual bottle for each vertical. 	However, additional sediment bottles must be used to avoid overfill. If more than one sediment 	bottle is needed, please request that they be combined at the sediment lab for a single sediment 	analysis.  Refer to SIR 2005-5077, Introduction to Suspended-Sediment Sampling by Nolan, 	Gray, and Glysson for a review of the USGS sampling methods for suspended sediment. This is a 	tutorial presentation that can be burned to a CD/DVD and run on a Windows-based PC.

Equipment used for compositing samples
Protocol requires the use of protected environments for processing and preservation of water-quality samples in order to reduce the possibility of contamination. They can be easily constructed with several plastic bags and a plastic milk crate, or a frame built with PVC tubing.
· Two types of compositing vessels will be used in general, depending upon the constituent-
1. churn splitter for major ions and alkalinity, nutrients, carbon, and isotopes samples
· to reduce the potential for contamination from atmospheric inputs, the plastic churn splitter must be modified with a plastic (polyethylene or polypropylene) funnel in the lid capable of being capped)
· this funnel is usually made by cutting off the bottom section of a 1-liter sample bottle and inserting the top into a 1-inch hole drilled into the lid of the churn splitter; the bottom is used for the funnel cap
· as a further precaution against contamination, the churn splitter should be placed inside two large, clear plastic bags which are kept closed except when adding sample to the churn
· the churn, inside the plastic bags, is then placed inside a large, covered plastic container (i.e. garbage can) which serves as the churn carrier
· this churn should not be rinsed with methanol
2. Teflon® churn splitter (8-L or 14-L), 3-Liter Teflon® bottle, or glass carboy for pesticide samples. 
· wrap the cork or rubber stopper with aluminum foil if using a glass carboy.
· Because the churn splitter has been approved for processing whole-water samples only when concentrations of suspended sediment do not greatly exceed 1,000 mg/L, the cone splitter is recommended for use at a small number of stations where these sediment concentrations are observed. If logistical concerns preclude the use of the cone splitter at a particular site, however, the rationale for the decision must be documented and the churn may be used. Consult National Field Manual Ch. 5.1.1.B for further details on the use of the cone splitter
Filtration of samples
· Inorganic Samples -- a variable-speed pump fitted with a peristaltic pump head that forces the sample through either C-Flex (inorganics)  and a GWV capsule filter system (effective pore size of 0.45 µm) (available from the National Field Supply Service through One-Stop Shopping as item Q398FLD).
· Pesticide samples—the new pesticide schedule 2437 has replaced schedule 2033. The new schedule uses the plastic syringes and 25mm 0.7 um glass-fiber syringe disk filters. See Attachment 7 for details on processing the schedule 2437 samples.  
· Particulate carbon and nitrogen (National Field Manual 5.2.2.C)—the polysulfone filter funnel or FEP pressure-filtration assembly (Q444FLD) that holds a 25-mm glass fiber filter (nominal pore size of 0.7 µm) (available from the National Field Supply Service through One-Stop Shopping as item Q441FLD).
· Dissolved carbon (organic and inorganic) and nitrogen,  and UV samples—the  GWV capsule filter system (available from the National Field Supply Service through One-Stop Shopping as item Q398FLD) or FEP pressure-filtration assembly (Q444FLD) that holds a 25-mm glass fiber filter (nominal pore size of 0.7 µm) (available from the National Field Supply Service through One-Stop Shopping as item Q441FLD).

Equipment cleaning

Cleaning procedures are described in detail in Chapter 3 in the National Field Manual. Briefly, they include the following--
· use of gloves, which are changed between each step
· 30-minute soak in Liqui-Nox (0.1% solution), or other phosphate-free detergent, followed by scrubbing with a nonmetallic, noncolored brush (except for the organic carbon filtration unit and Teflon equipment, unless deemed necessary because of exposure to high concentrations of organic carbon)
· thorough rinsing with hot tap water
· final rinses:
1. sample bottle, cap and nozzle
· 30-minute soak in a solution of 5% hydrochloric acid (trace-element grade)
· three rinses with DIW
· rinse with a small amount of methanol (pesticide grade) but sufficient to contact all sample contact surfaces
· cover and allow to air dry completely
· assemble sampler and wrap nozzle with aluminum foil
· double-bag
2. churn or cone  splitter and associated tubes and pump tubing –note the churn spigot should be removed and cleaned separately after the final soaking of the churn.  The Teflon spigot should be completely disassembled before cleaning.
· 30-minute soak in a solution of 5% hydrochloric acid (trace-element grade)
· three rinses with DIW
· double-bag
3. glass carboy (or Teflon® churn splitter or Teflon® bottle)
· Detergent wash
· Tap water rinse
· rinse with a minimal amount of methanol (pesticide grade).  DO NOT RINSE THE DOC PROCESSING EQUIPMENT WITH METHANOL.  
· Air dry, wrap with aluminum foil and/or double-bag
4. TPCN equipment
· thoroughly rinse with DIW
· DO NOT RINSE WITH METHANOL.  

· rinse all inorganic sample bottles three times with DIW, then half-fill with DIW for transport to the field
Field analyses
Complete descriptions of standard protocols for field measurements are provided in Chapter 6 of the National Field Manual.
Specific guidelines for the NFSN program include the following:
· Obtain a cross-section stream profile of field measurements at least twice/year
· record observations from at least three depths in the cross section
· repeat during the year under different flow conditions.
· code these measurements as follows--
· medium=WSQ (QC sample)
· stype=B (other QA)
· Routine measurements
· water temperature and dissolved oxygen should be measured directly in the stream (see National Field Manual Ch. 6.1 and 6.2)
· specific conductance and pH can be measured in the stream or from an unfiltered sample from the churn splitter (see National Field Manual Ch. 6.3)
· alkalinity, bicarbonate, and carbonate concentrations are measured using a filtered sample as soon as possible after sample collection is complete, using the incremental advanced speciation method of alkalinity determination with the digital titrator (see National Field Manual Ch. 6.6) http://water.usgs.gov/admin/memo/QW/qw12.05.pdf
· Record all expiration dates and lot numbers of pH buffers and specific conductance standards on the field form and in NWIS

Collection methods
A complete description of sample collection guidelines is provided in Chapter 4 of the National Field Manual.
· Overview of multi-vertical, depth-integrated sampling for water-quality constituents:
· EDI method is suitable for rivers with well-defined and relatively stable discharge patterns and streambeds
· EWI method is preferable for wadeable streams or large rivers with unstable streambeds
· rinse all sampling equipment thoroughly with river water prior to collecting the first sample
· Rinse the sampler 3 times with native water; about 200 ml for rigid bottles and about 20% of total volume for bags.
· Rinse the churn splitter once; with 2 liters from the sampler for the 8-Liter churn and with 4 liters from the sampler for the 14-Liter churn.
· Rinse the cone splitter with 2-4 liters of native water from the sampler
· if possible, collect samples at the same cross section throughout the period of record (may not be possible if station is wadeable during part of the year, and sampled from a bridge or cableway during the rest of the year)
· the number of verticals should be based primarily on the requirement to collect a representative sample of the cross section.  The minimum number of vertical stations is 10 for EWI and 5 for EDI
· the vertical transit rate and operational depth for the DH-81 is a function of the stream velocity, sample-container volume, and nozzle size—
		---------------------------------------------------------------------------
			Sampler	Nozzle diameter	Ratio	Depth
				     (inches)		(feet)
		---------------------------------------------------------------------------
			DH-81	3/16		0.1	wadeable
				1/4		0.2	wadeable
				5/16		0.4	wadeable
		---------------------------------------------------------------------------
		     Stream velocity x ratio = maximum vertical transit rate.
		---------------------------------------------------------------------------
The D-96 is not subject to the same transit rate limitations of rigid bottle samplers. The minimum transit rate is one at which the sample volume does not exceed 3 L. The sampling time for the three diameter nozzles at varying stream velocities is given in USGS OFR 2005-1087 (Davis and FISP, 2005) that describes the D-96 sampler. The minimum transit rate can be calculated using the sample time from the table and the total distance to be transited.
Complete depth- and width-integrated samples are collected for suspended sediment and percent fines as part of the routine NFSN sample trip. 
Composite samples are collected for splitting into sub-samples for all other constituents, as described below:
· Compositing with the churn splitter
· in order to obtain a sample for DOC/PC which is representative and comparable to other constituents, assuming ongoing acceptable results are obtained from laboratory blank samples for DOC, this sample will be collected using the same sampler and collection method as the inorganic water-quality samples and composited into a splitter not rinsed with methanol.
· A total of three to four passes are necessary at each vertical in the cross section, collected into different sets of containers. Whenever conditions allow, rotate the order of sample collection for specific analytes.  Rotating the order of sample collection is especially beneficial if the hydrologic condition is changing (falling or rising stage) during sample collection. Collect samples as close in time as possible in an order similar to the following:
1. First sample station:
· suspended-sediment
· churn splitter (inorganics and DOC/PC)
· glass carboy (or Teflon® churn splitter) for pesticides
2. Second sample station:
· churn splitter (inorganics and DOC/PC)
· glass carboy (or Teflon® churn splitter) for pesticides
· suspended-sediment 
3. Third sample station:
· glass carboy (or Teflon® churn splitter) for pesticides
· suspended sediment
· churn splitter (inorganics and DOC/PC)
4. Fourth sample station: repeat first station, etc.
· Compositing with the cone splitter
· A whole water sample is required for inorganics and DOC/TPCN but not for pesticide sample.   Two to three passes are necessary at each vertical in the cross section and collected into different sets of containers as follows--
1. Plastic, glass, or Teflon®  bottles that have not been rinsed with methanol for inorganics and suspended-sediment 
2. Glass carboy or Teflon®  churn for pesticides, Teflon® containers for pesticides
[bookmark: HDR6]Sample processing
Complete descriptions of sample processing details are provided in Chapter 5 of the National Field Manual.
· Filtration guidelines:
· Withdraw samples for whole-water constituents and particulate carbon first. 
· Record all expiration dates and lot numbers for filters on the field form and in NWIS
· Specifics on procedures for particulates—
· Particulate carbon and nitrogen
· a total of three filters are required to be sent to the NWQL for analysis of particulate carbon and nitrogen
· the pressure must be regulated to less than 15 lb/in2
· each filter, after drying as much as possible, is carefully removed, folded in half with the sediments inside, and placed on a 6-inch square of aluminum foil; after the volume of sample that passed through the filter is recorded on the foil and in comments to NWQL on ASR, it is folded and double bagged into sealable bags
· samples for the NWQL should be shipped as soon as possible
· Inorganic constituents, dissolved organic and inorganic carbon, and UV absorbance
· Capsule filters are used for the filtration of dissolved nutrients, major ions, and alkalinity samples as well as DOC, DIC, and UV if so desired.
· the filter must be  preconditioned (with 50 mL DIW (deionized water) if using the low-capacity capsule (Aquaprep) or the 25mm filter, or with 2 liters DIW if using the large-capacity filter ), using the pump to drain the water remaining in the filter as much as possible
· sample bottles should be rinsed and filled from the capsule filter in the following order:
· Rinse and fill the FA bottle first. Use no more than 100 mL of filtered water to rinse the remaining sample bottles (that require rinsing)
· fill the remaining bottles in the following order: nutrients (FCC), anions (FU), alkalinity (FU), DIC, UAS, DOC 
· Use the Teflon® pressure-filtration assembly that holds a 25-mm glass-fiber filter for the DOC sample or use approved low or large capacity capsule-filter type. (see Office of Water Quality-Information Notes http://water.usgs.gov/usgs/owq/WaQI/index.html), particularly Note 2009.10. Do not rinse the sample bottle. 
· Also note: if the DOC samples are filtered with the 25-mm glass-fiber filters, the lab code for the DOC sample must be changed. The lab code has changed from LC2612 to LC2613. Please delete LC2612 and add LC2613 to the lab code list in the Analytical Work Request Section of the ASR.
· DIC sample - do not rinse the sample bottle, do not add sulfuric acid preservative, and do not leave headspace. Use the same filtration options used for the DOC sample. 
· UV sample (UAS bottle) -Because the DOC sample requires acidification (see below), a separate bottle must be filtered for the UV absorption sample (see NWQL Policy Memo 2000.04)
· 60 mL is a sufficient volume for the UV sample, filtered into a baked-glass amber DOC bottle
· Label bottle ‘UAS’ and the appropriate nutrient schedule number (SH2430 or SH2431 or SH2432) on the bottle label.
· The UV-254nm and UV-280 nm absorption analytes require a different lab code when using the 25mm glass-fiber filters. (A similar problem we have with the DOC samples). Note: The UV-412nm absorption analyte does not require a different lab code when using the 25mm glass-fiber filters. 
If using the 25mm GFF for processing the UV samples
· On the ASR - delete LC2616 (UV 254nm) and LC2617 (UV 280nm) then add LC2614 (UV 254nm) and LC2615 (UV 280nm)

· Preservation
· the FA bottle for schedules 998/1201 is preserved with 2 mL of 7.5-7.7 Normal Ultrex-grade nitric acid, provided in polypropylene vials (see National Field Manual Ch. 5.4 for more information). The pH of the preserved sample must be <2.
· samples for whole-water nutrients (WCA bottle) and dissolved organic carbon (DOC bottle) are preserved with 1 mL of 4.5 normal sulfuric acid (see and NWQL Policy Memo 2000.04 for more information
· all nutrient and organic samples are stored at 4oC
· Record all expiration dates and lot numbers for acids on the field form and in NWIS

Information on the following analytes is currently not available in the NWQL catalog. Contact Dave Reutter if additional information is needed.
· Dissolved Inorganic Carbon (DIC) – Filter sample using either a 25mm glass-fiber filter or a capsule filter into a 125-ml amber glass bottle baked at 450 degree C (same bottle type used for DOC samples). Do not rinse bottles but rinse filter with organic-free water. Do not add sulfuric acid preservative, do not leave headspace. Chill and maintain at 4 degree C, ship immediately. If using a glass-fiber filter, it may be retained for Total Particulate Carbon or Particulate Inorganic Carbon analysis. Include ‘DIC’ and the appropriate nutrient schedule number (SH2430 or SH2431 or SH2432) on the bottle label.
· UV 412nm – no additional sample processing is required for this constituent as an aliquot for analysis of this constituent will be taken from the same bottle used for analysis of UV254 and UV280. Label the UAS bottle ‘UAS’ and the appropriate nutrient schedule number (SH2430 or SH2431 or SH2432) on the bottle label.
· Pesticides -- Please refer to Attachment 7 for details on processing Schedule 2437 samples.

· Shipping
· A detailed description of shipping requirements is provided in NWQL Technical Memorandum 02.04 [http://nwql.usgs.gov/Public/tech_memos/nwql.02-04.html]
· All sample bottles must be clearly labeled with pre-printed labels or a waterproof marker with the following minimum information--site identification number, date, time, and sample designation code
· Particulate carbon and nitrogen 25 mm filters can be placed in a sealable bag in with ASRs as an added protection from melted ice.
· Include a NWQL Analytical Services Request (ASR) Form for each sample sent to the laboratory, retaining a copy; place the ASR form inside a sealable plastic bag and tape the bag to the inside of the cooler lid

Funds for sample and cooler shipments have been provided to the WSCs. Do not use any headquarters account for shipping samples.

Important!  Ship chilled sample containers in coolers packed with sufficient ice to maintain a temperature at or below 4ºC.  The NWQL has recently received a number of warm coolers. Samples that should be shipped chilled, but arrive at the lab warm, should be discarded. Please contact Dave Reutter (dreutter) if contacted by the NWQL because of warm samples.
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Attachment 3.  QW Sample Coding Guidance
Complete water-quality sample coding information can be found at: 

https://internal.cida.usgs.gov/wiki/display/nawqadatasynth/complete+descriptive+version

Environmental Samples

(1) Analytical Services Request Forms

Sample Time        Time of collection, rounded to nearest 10-minute interval                     
Sample medium   WS (surface water)      
Sample type           9    (regular)	
Program/Project         SWMSA (NAWQA)
		  NASQAN 
		  NMN	

(2) QWDATA

Parameter                                		 Primary sample
Time        				Time-of-collection, rounded to 10-minute interval
Sample medium   			WS (surface water)
Sample type 			9 (regular)
    Note: Sample type will be 7 (replicate) if there is an associated secondary replicate sample

71999 (sample purpose)		    15 (NAWQA)
				    20 (NASQAN)
				    25 (NMN)

50280 (purpose of site visit)		1001 (Fixed frequency)

99111 (QC sample associated)		      1 (No associated QA data)
				    10 (Blank)
				    30 (Replicate sample)
				    40 (Spike)
				  100 (More than one type of QA sample)
			

Also include sampler type (parameter code 84164), sampling method (parameter code 82398) and splitter type (parameter code 84171) when logging in samples. Coding for these parameters are found at: http://waterdata.usgs.gov/usa/nwis/qwdata?codes_table26_help


Blank Samples

(1) Analytical Services Request Forms

		Environmental		Field blank

Time		Time of collection		8 minutes after
		rounded to nearest		environmental
		10-minute interval		sample time
Sample medium	WS (surface water)		OAQ (QA, artificial)
Sample type	9 (regular)		2 (blank)
Analysis Status	U (unrestricted)		I (internal-use only)
Login comment: Field blank prepared before sampling; equipment last used at station ID on date; blank water lot number ____

(2) QWDATA

Parameter				Environmental sample

99111 (QA data associated w/sample)	    10 (blank)
71999 (sample purpose)		    15 (NAWQA)
				    20 (NASQAN)
				    25 (NMN)


				Blank sample

71999 (sample purpose)		    15 (NAWQA)
				    20 (NASQAN)
				    25 (NMN)

50280 (purpose of site visit)		1098 (QC sample)

99100 (type of blank solution)		   40 (Pesticide/DOC grade organic-free water)
				   10 (IBW/inorganic grade water)
				 110 (both IBW & Pest/DOC grade OFW) Note: Please avoid collecting the inorganic blank and the organic blank samples during the same sampling trip.


99101 (source of blank solution)		  10 (NWQL)
99102 (type of blank sample)			 100 (field)
					 150 (lab)
					      1 (source)
					    40 (sampler)
					    50 (splitter/tubing)

Coding of Blank Water Lot Numbers
    99200 (Inorganic Grade) see list of IBW lot numbers at http://wwwnwql.cr.usgs.gov/qas.shtml?ibw

or
   99202 (Pesticide Grade) see list of OBW lot numbers at http://wwwnwql.cr.usgs.gov/qas.shtml?obw



Replicates (NWQL and Suspended Sediment Samples)

(1) Analytical Services Request Forms

                              Primary                                        Secondary

Time                     Time of collection                       One minute later
                              rounded to nearest                       than primary sample
                              10-minute interval
Sample medium    WS (surface water)                      WSQ (QA, surface water)
Sample type          7 (replicate)              	                 7 (replicate)
Analysis Status	U (unrestricted)		I (internal-use only)


(2) QWDATA

Parameter				Primary			Secondary

99111 (QA data associated w/sample)	30 (replicate)		--
99105 (replicate type)		10 (concurrent)   or		10 (concurrent)   or
				30 (split)			30 (split)
71999 (sample purpose)		15 (NAWQA)		15 (NAWQA)
				 20 (NASQAN)		20 (NASQAN)
				 25 (NMN)		25 (NMN)

50280 (purpose of site visit)		1001 (Fixed Frequency) 	1098 (QC sample)



Also enter sampler type (parameter code 84164), sampling method (parameter code 82398) and splitter type (parameter code 84171) when logging in samples. Coding for these parameters are found at: http://waterdata.usgs.gov/usa/nwis/qwdata?codes_table26_help

Pesticide field spikes
(1) Analytical Services Request Forms

                Environmental                              Spike

Time       Time of collection                      Three minutes after
                rounded to nearest                      environmental
                10-minute interval                     sample time
Sample medium   WS (surface water)      WSQ (QA, surface water)
Sample type          9 (regular)		1 (spike)
Analysis Status    U (unrestricted)	I (internal-use only)

(2) QWDATA

Parameter                                 Primary sample

99111 (QA data associated w/sample)    40 (spike)
99106 (spike type)                                    10 (field)
71999 (sample purpose)                           15 (NAWQA)
			                20 (NASQAN)
			                25 (NMN)
50280 (purpose of site visit)		1001 (Fixed Frequency)

                                              Secondary sample

99106 (spike type)                         	10 (field)
99104 (lot number)          		see list of spike lot numbers at http://wwwnwql.cr.usgs.gov/qas.shtml?spike#LS2437

99107 (spike source)                     	10 (NWQL)
99108 (spike volume)                   	0.1 (mL)
71999 (sample purpose)                	15 (NAWQA)
			                20 (NASQAN)
			                25 (NMN)

50280 (purpose of site visit)		1098 (QC Sample)


Login comment: Field spike for S2437 for station ID on date/time;
spike lot number is _____.

Note: Normally, spikes are collected during the non-growing season. If taken during the growing season, a higher spike volume may need to be added to the sample.

Attachment 4.  Guidelines for Collection of NFSN QC Samples

The collection and evaluation of QC samples are essential elements of the NFSN program, which contains a strong interpretive component. Without QC information, the quality of the environmental data cannot be evaluated or qualified, limiting the interpretive value of the data.
Objectives of the QC sample analysis include the following--
· to determine the extent of contamination introduced from the equipment and methods used for sampling and processing
· to provide information about the variability and bias of measured concentrations
· to evaluate the effect of the natural-water matrix on the bias and recovery of measured concentrations for selected analytes
QC samples for NAWQA include field-equipment blanks, replicates, and field-matrix spikes. Consult the NFSN SWPLAN for information on the QC samples required of the individual NFSN sites in 
FY 2014.
Field blanks
A field blank is a blank solution that is generated under actual field conditions and is subjected to the same aspects of sample collection, field processing, preservation, transportation, and laboratory handling as the environmental samples.
Field blanks should be prepared immediately before collecting and processing a native-water sample at a selected site.
· equipment should already be pre-cleaned in preparation for the routine environmental sampling
· it is not necessary to clean the equipment after sampling and processing of the field blank before using it to collect and process the environmental sample
· field blanks will be required for all constituents except suspended sediment
· The procedures used to process the field blank should, with few exceptions, be the same procedures used to collect and process the environmental sample
· beginning this year, use the same lab schedules for field blanks that are used for the environmental samples --
   Schedule(s)          	          Analysis                      Blank Water         Delete these lab codes on ASR
							
2430 or 2431 or 2432        Nutrients                      	Inorganic		2612, 2616, 2617, 8096
							

998 or 1201                        Major ions                   	Inorganic

2437             	          Pesticides                        Organic

Lab Codes

8096         	          DOC		Organic
2612, 2616, and 2617        UAS		Organic					

The bottle requirements for these schedules can be found in the NWQL LIMS Catalog http://wwwnwql.cr.usgs.gov/USGS/catalog/index.cfm 
Approximately two to three gallons of blank water (either inorganic- and organic-free) with the same lot number are required for adequate rinsing and processing.
· Because of the potential for contamination, a field blank should be prepared using either inorganic- or organic-free blank water, but not both during the same site visit.
· blanks (see Chapter 4.3.1.B of the National Field Manual) for inorganic constituents (WCA, FCC, FA, FU, RU, and DIC samples) should be prepared as follows:
· collect two initial samples of the source solution one for each schedule if necessary
· The following steps should be accomplished outside the mobile laboratory:
· rinsing of the sampler should simulate as closely as possible the field rinsing that occurs prior to collection of the environmental sample
· after the initial rinsing with blank water, fill the sampler bottle or bag and pour through the nozzle into a sample bottle for the sampler blank
· fill sample bottle or bag with blank water and empty through the nozzle into the churn until it contains 2-4 liters of blank water.
· Rinse and empty the churn completely from the spigot
· pour the remainder of the blank water from the sampler into the churn splitter; refill the sampler and repeat until the churn contains about 5 liters of water;  
· collect a splitter blank from the churn while churning
· pump an aliquot of blank water from the churn splitter, using the routine pumping system, into a sample bottle for the pump blank
· pump an aliquot of blank water from the churn splitter through the preconditioned filtration system (with 100 mL IBW if using the low-capacity capsule filter (Aquaprep) or the 25mm filter, if using the large-capacity filter 2-L DIW (deionized water) into a sample bottle for the field blanks
· preserve all samples as required; submit only the final field equipment blank samples to the laboratory and store the remainder of the samples appropriately (chilled if necessary) for later analysis, if necessary. 
· field  blanks for TPCN samples: 
· Only a final blank should be processed for the TPCN sample. Charlie Patton (NWQL) has asked that a standardized volume of IBW used for the TPCN field blanks. Please use 125-ml of IBW per filter for the TPCN field blank samples.
· blanks for UAS and PEST samples (organic constituents) should be prepared as follows:
· collect initial samples (40-ml vial and a 125-mL amber glass bottle) of OBW for the source solution
· The following steps should be accomplished outside the mobile laboratory:
· rinsing of the sampler should simulate as closely as possible the field rinsing that occurs prior to collection of the environmental sample
· after the initial rinsing, fill the sampler bottle or bag with blank water and pour through the nozzle to rinse and fill a sample bottle for the sampler blank
· fill and rinse the glass carboy or Teflon® churn splitter from the sampler; refill the sampler and repeat until the carboy/churn contains at least 2 to 3 liters of water; 
· remove an aliquot of blank water from the glass carboy/churn and filter the blank water as described in attachment 7 for the pesticide blank
· after conditioning the capsule filter (with 50 mL OBW if using the low-capacity capsule filter (Aquaprep) or the 25mm filter; if using the large-capacity filter, 2L DIW), filter an additional 100 mL from the churn splitter and submit the filtrate for the UV field blank.
· blanks for DOC samples (organic constituent) should be prepared as follows:
· collect an initial sample (a 125-mL amber glass bottle) of OBW for the source solution
· The following steps should be accomplished outside the mobile laboratory:
· rinsing of the sampler should simulate as closely as possible the field rinsing that occurs prior to collection of the environmental sample. This is especially important for DOC samples if the sampler is rinsed with methanol. 
· after the initial rinsing, fill the sampler bottle or bag with blank water and pour through the nozzle to rinse and fill a sample bottle for the sampler blank
· use a churn that has not been rinsed with methanol. Fill and rinse the churn splitter from the sampler; refill the sampler and repeat until the churn contains at least 2 liters of water; 
· after conditioning the capsule filter (with 50 mL OBW if using the low-capacity capsule filter (Aquaprep) or the 25mm filter; if using the large-capacity filter, 2L DIW), filter an additional 100 mL from the churn splitter and submit the filtrate for the DOC field blank.

If the data from the laboratory fall within the QC requirements (described below), the field blank is acceptable and the other samples may be discarded.
· If all or some of the data exceed the acceptable levels, further investigation will be required to determine the source of the contamination. 
Quality-Control Requirements
Acceptable concentrations for the equipment blank for inorganic constituents and pesticides are either less than or no higher than the MDL (minimum detection limit) + 100 percent. Concentrations higher than this must be evaluated in context with environmental data, and may still be considered acceptable.
Blanks for organic carbon are considered acceptable if concentrations are either less than or no higher than twice the MRL (0.15 mg/L). Concentrations higher than this must be evaluated in context with environmental data, and may still be considered acceptable.
Consult the sample coding guidelines document for completing ASR's and entering data into QWDATA.
Replicates 
Concurrent replicates are two or more samples that are collected as closely as possible in time and space, but processed, handled, and analyzed separately; these samples provide information about the total variability inherent in the observed concentrations, including sampling, processing, and laboratory variability.
· collection of concurrent replicate samples requires two separate passes for the particular suite of constituents at each vertical in the cross section, composited in separate compositing vessels
· collect a second set of field parameters and enter them into NWIS.  DO NOT ENTER THE SAME FIELD PARAMETERS VALUES FOR BOTH SAMPLES UNLESS THEY WERE THE ACTUAL MEASUREMENTS.
Consult the sample coding guidelines document for completing ASR's and entering data into QWDATA.
Field-matrix spikes
Environmental sample fortified in the field with known concentrations of all, or a representative selection of, the analytes for a particular method; this sample must be submitted along with a split sample which is not spiked
· field matrix spikes (supplied by NWQL) will be collected only for pesticides (Schedule 2437).
Detailed instructions for using the pesticide spike mixture for S2437 are provided with the spike mixture (500 microliters in a 1 mL ampule), along with 100 microliter micropipets and a Teflon® squeeze bottle
· the ampule should be kept in the freezer if long-term storage is required
Consult the sample coding guidelines document for completing ASR's and entering data into QWDATA.
Contact Dave Reutter (dreutter, 614-430-7732) regarding questions about QA/QC sampling and review of QC data.
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Attachment 5: Review of Ecological Data in BioData

Annual review of ecological data collected in CY2013 is the responsibility of the Science Center (SC) that was responsible for collecting the samples.  Data review is to be completed for all samples collected in CY2013, including sites that have not been retained as part of the Cycle 3 National Fixed-Site Network.  Science Centers should continue to maintain legacy data originally entered into BioTDB and resolve any errors or warnings that remain in those data, especially data from Cycle 2.

1. ACTION: By January 15, 2014; enter into BioData all field data for macroinvertebrate, algae, fish, and habitat samples collected during CY 2012. Entering data into BioData promptly when returning from the field will make it easier to resolve problems before they impact laboratory analyses and data users.  Data entry and initial review of all CY2013 data in BioData is to be completed by January 15, 2014; also be sure that all data collected in previous years (including taxa ID/count records) have been entered and/or reviewed.

Guidance for ecological data review in BioData is available at: https://my.usgs.gov/confluence/display/biodata/Data+Review+Guidance.  Review steps described in this guidance include:
Step 1 - Review Your Project Profile
Step 2 - Review Your Study Reaches
Step 3 - Review Your Physical and Community Samples
·	Using the Physical or Community Sample Tab to Determine Review Status
·	Using the Data Release Status Tab to Determine Review Status
·	Using the Sample Data Entry Screen to Determine Review Status
Step 4 - Review Your Taxa ID/Count Records.

For questions about data review requirements for NAWQA data, contact Amanda Bell (ahbell@usgs.gov).  To obtain assistance, guidance, or clarification of BioData review procedures, contact Mitch Harris (maharris@usgs.gov) or Pete Ruhl (pmruhl@usgs.gov). 

2. ACTION: By April 15, 2014 repeat the data review steps in BioData and confirm that all problems have been resolved for samples collected during CY2013 or earlier.
Periodic review of the issues raised by the data checking subsystem is necessary to ensure that the NAWQA databases are well-maintained. Failure to review data by this date will be reported to the SC’s Director, RNPO, and REX.

3. ACTION: Review all algal and invertebrate taxonomic data released by laboratories within 3 months of the date they were loaded into BioData, or April 15, 2014, whichever is sooner.
Note that project owners will receive an email alerting them when data are loaded. Data from samples collected during CY2013 that have not been loaded by April 15, 2014, are to be reviewed within 3 months of the date of loading; also review taxonomic data from samples collected prior to 2013 that have not yet been reviewed. Tip: the Data Release Status tab in BioData can be used to find samples that have taxonomic lab data that are awaiting review. 




Attachment 6: Fish Quality Assurance Plans

REMINDER: Fish Quality Assurance (QA) Plans are required from all Science Centers responsible for collecting NAWQA fish community samples.  Once submitted, each plan is to be updated annually with information about collecting permits and noting any changes in: (1) the individual(s) responsible for making taxonomic identifications in the field and laboratory, (2) locations of vouchered specimens, (3) status of listed species, (4) status of electrofishing certification and CPR training for personnel involved in sampling, or (5) other changes that may significantly affect fish collection. Updates are to be sent electronically to Mike Meador (mrmeador@usgs.gov).  Please submit an updated plan each year by April 15, 2014, even if there have been no changes.   

Information regarding the creation and maintenance of the QA plans can be found in Walsh and Meador (1998) located at http://water.usgs.gov/nawqa/protocols/WRI98-4239/index.html. An entry should be made in the SWPLAN spreadsheet each year to indicate that the plan has been submitted for that year’s sampling effort, for any site where fish collections are scheduled.

The table below indicates the most recent version of a Fish QA Plan submitted by Cycle 2 study units that collected fish community samples in 2013; many of these plans have not been recently updated.  For Cycle 3, only one Fish QA Plan needs to be submitted per Science Center.  Please ensure that updated plans are submitted by any SC responsible for conducting NAWQA fish-community sampling in FY14. 

	Region
	SC
	SUID
	DATE

	CR
	LA
	ACAD
	5/30/2013

	CR
	NE
	CNBR
	4/12/2013

	CR
	IA
	EIWA
	3/21/2013

	CR
	AR
	OZRK
	4/10/2013

	CR
	NM
	RIOG
	4/17/2013

	CR
	TX
	SCTX/TRIN
	4/15/2013

	CR
	CO
	SPLT
	2/8/2013

	CR
	MN
	UMIS
	5/7/2013

	CR
	WY
	YELL
	4/18/2013

	NR
	CT
	CONN
	2/25/2013

	NR
	NJ
	DELR
	5/11/2012

	NR
	NY
	HDSN
	4/17/2013

	NR
	OH
	LERI
	4/12/2013

	NR
	NJ
	LINJ
	7/18/2003

	NR
	MD-DE-DC
	PODL
	4/18/2013

	NR
	IL
	UIRB
	6/15/2005

	NR
	IN
	WHMI
	3/19/2013

	NR
	WI
	WMIC
	4/17/2013

	SE
	GA
	ACFB
	4/16/2013

	SE
	NC
	ALBE
	2/8/2013

	SE
	AL
	MOBL
	4/11/2013

	SE
	SC
	SANT
	4/16/2013

	SE
	TN
	TENN
	7/5/2005

	SE
	MS
	
	4/11/2013

	WR
	AZ
	CAZB
	4/9/2013

	WR
	WA
	PUGT
	3/20/2013

	WR
	UT
	GRSL
	5/2/2013

	WR
	CA
	SACR/SANJ/SOCA
	2/12/2013

	WR
	ID
	USNK
	11/19/2013

	WR
	OR
	WILL
	6/7/2013
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Attachment 7: Field and Processing Protocol for Pesticide Method Schedule 2437 
	

Background

The National Water Quality Lab (NWQL) has developed a new method for pesticide analysis which requires a low-volume sample. The new pesticide method will be requested as NWQL Schedule 2437.

This new pesticide filtering method will save time during sample processing, and should also reduce other preparation time by eliminating the amount of equipment used, and cleaning time. The FMI pump, corrugated Teflon tubing, aluminum filter plate, and 142-mm GF/F used for Sch 2033 and Sch 2060 will be replaced with a 30-mL syringe constructed of high purity polypropylene and polyethylene , a blunt large bore needle, and 25-mm diameter 0.7 um GF/F disk syringe filters. The syringe, syringe filter, and needle are discarded after use. The new method will only require a 20-ml sample in a 40-ml GCV vial (One Stop N1560). [Note: once this method is approved, only 10-ml will be required, in a 20-ml GCV vial.]

[image: ][image: ]


Instructions for the collection and processing of these new samples are provided below. If you have questions, please contact Dave Reutter (614-430-7732 or email dreutter).



Field Procedures

Collection

1. Collect your samples as you usually would, as described in the standard methods. 

Processing

As per the NFM (Chapter 5.2.2) “CH/DH techniques and associated QA procedures for inorganic analytes with parts-per- billion concentrations are not required for organic analytes but are recommended as good field practices to maintain the integrity of sample chemistry. Field personnel must wear disposable, powder-free gloves.



1. At the field site, cover the field bench or work area with a clean sheet of aluminum foil to prepare a clean work surface. Place plastic bag containing syringe, large bore needle, and disposable filter near the clean work surface. Change gloves.

2. Remove syringe, large bore needle, and syringe disk filter from the bag and its wrappings, and place on the clean foil. Attach needle to Luer-Lock fitting on syringe (The open female end of the syringe is twisted onto the male Luer-Lock fitting on the syringe to provide a secure fit).

3. Homogenize the composited pesticide sample in your standard manner.

A. If you usually use a glass carboy for your pesticide sample, you’ll have to pump (using the FMI pump and tubing only) a raw, unfiltered subsample into a suitable container for pesticide analysis (such as a 125-ml glass baked amber bottle) for syringe filtering. The bore needle will not reach the bottom of this bottle, and refilling will be necessary throughout the process. Note: For field crews that will continue to use a glass carboy for their pesticide samples – Please contact Dave Reutter if you plan to continue using the glass carboy. Mark Sandstrom has identified tubing connectors that allow the Luer-Lock to be fitted directly to the tubing. This would eliminate the need for the syringe and needle, but would require these additional fittings to be cleaned after each use as well as the pump and tubing (see details at end of this attachment ‘Reducing Fittings for Syringe-tip filters for Surface-water samples’). 

B.  If you usually use the Teflon churn as your pesticide compositing device, you can withdraw the sample directly from the churn using the syringe and bore needle.

4. Rinse syringe, bore, and filter. Submerse the bore needle into the subsample or the churn and withdraw 10-mL of sample through the needle into syringe. Invert syringe, pull stopper to the 30-mL mark on the syringe and shake, ensuring full rinse of the syringe. Depress plunger, expelling water into a waste container. Again, submerse the attached bore needle into the subsample or churn, and withdraw 5-mL of sample into the syringe. Invert syringe and carefully remove needle. Place needle on clean piece of aluminum foil. Attach the filter to the syringe by pushing straight down and twisting until the filter is firmly in place on the syringe mechanism.

Invert syringe and slowly depress the plunger to force the sample water out of the syringe, through the filter to rinse the filter with sample water and expel the rinse water into a waste container. This completes the cleaning and conditioning steps.


5. Remove the filter and place on clean aluminum foil. Carefully reattach the needle to the syringe, and withdraw sample from the subsample as stated above, filling to the 30-ml mark.

Invert syringe, while tapping and depressing plunger to expel air, push the plunger to about the 25-mL mark. Remove needle and attach rinsed filter. Invert syringe downward, and Filter 20-ml into a 40-ml glass vial by depressing the plunger slowly.

 To collect as closely to 20 ml as possible, it is suggested to move the plunger from the 25-ml mark to the 5-ml mark. (expel the remaining 5-ml to waste).

Note: In the event that samples have extremely high suspended sediment, organic blank water (OBW) may be used to rinse and condition the filter instead of the 5 ml sample. If OBW is used for rinsate, the OBW rinse must be followed with at least 2mL of sample water (before collecting sample) to remove any remaining OBW. Pre-tests have shown that most high sediment sites can filter at least a 30-ml sample using this filter. If the syringe filter medium becomes clogged before a sufficient amount of sample has been filtered, re-filter with a new, conditioned filter by repeating steps 4 and 5 as necessary until at least 20-mL have been collected. These additional steps must be documented on the field sheets.



6. Label the vial with the appropriate station ID, date, time, and schedule number. Ensure caps are on firmly. Do not freeze. Chill and maintain the sample at or below 4°C without freezing during storage and shipment.

7. Discard the needle, syringe and filter. The syringes can be put into a plastic recycling bin. On field forms and in the field notes, document the number of filters used for each vial and any problems you encountered.

8. Ship all pesticide samples overnight to NWQL along with your other samples.




ASR Forms

No changes will be necessary on the primary ASR for the environmental Sch 2437 sample. Continue to use the same ASR you normally use for your site(s).  List the container as ‘PEST’.



Sample Time 

Round the sample time for the primary environmental sample to the nearest 10 minutes, for example 0940, 1200, or 1320. This sample time will be used for the environmental Sch 2437 and your non-pesticide samples (nutrients, sediment, etc.).



Blank Processing

Field blanks should be processed using standard methods as stated in the National Field Manual (NFM) Chapter A4 (4.3.1). Blanks for S2437 should mirror those guidelines. Follow the procedures outlined in this document (steps 1-9), substituting OBW for environmental water. These blanks should be done in the field, but prior to collecting and processing the environmental samples. 

Field Spikes

Use the new 2437 spike mixture for Sch 2437 samples. Please record lot number and volume for each spike mixture within the field notes.



Sample Login


The following parameter codes should be added when logging the samples into NWIS: 


Spikes, and Spike Replicates

Pcode 71999 = Sample Purpose = either NAWQA = 15, NASQAN = 20, or NMN = 25 
Pcode 50280 = Purpose of Visit =1098 (QA/QC, surface water)
Pcode 99107 = Source of Spike Solution = 10 NWQL
Pcode 99106 = Type of Spike Sample = 10 Field
Pcode 99108 = Spike Volume = (ml) 100 u/L = .1 ml
Pcode 99104 = Spike Lot number = See Spike Kit for NWIS Lot number

Blank Coding

Pcode 71999 = Sample Purpose = either NAWQA = 15, NASQAN = 20, or NMN = 25
Pcode 50280 = Purpose of Visit =1098 (QA/QC, surface water)
Pcode 99100 = Type of Blank Solution = 40 Organic-Free water 
Pcode 99101 = Source of Blank Solution = 10 NWQL
Pcode 99102 = Type of Blank Sample = 100 Field
Pcode 99202 = Organic Blank Lot number = see container or NWQL web page for NWIS Lot number
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Equipment for Schedule 2437 


The orders can be made in no fewer amounts than 50 for syringes and needles, and 20 for filters. Keep this in mind when ordering supplies for more than one site- you may not have to order more than one bag of syringes or needles. 

In order to avoid contaminating the filtration supplies, it would be good practice to store the bags of needles, syringes 10/10/2012and filters in a clean area of the WSC laboratory. Transfer only as many supplies as needed for each sampling trip to a separate clean bag to take to the field vehicle.


You may order the following from USGS One Stop Shop:
· 1 case (72/case) 40-ml glass vials, GCV (Order from One Stop, N1560)
· Pesticide-grade blank water (Order from USGS One Stop, N1590)
· 1 bag (of 50) Plastic syringes (Order from One Stop Q763FLD)
· 1 bag (of 50) Large-bore needles (Order from One Stop Q764FLD)
· 1 bag (of 20) 25 mm 0.7 um glass-fiber syringe disk filters (Order from One Stop Q762FLD)
· 20-mL glass vial, PEST (should become available from One Stop when method is approved)

You may consider purchasing vial polyurethane foam or polystyrene shippers (similar to these: http://www.epscientific.com/product/environmental.aspx?id=38 ) to store and ship 20- and 40-ml vials.  

Sch 2437 spike mixture can now be purchased from One stop shopping, Item number N2437 ($36.00). Please order the spike mixture near the date that the spike sample is planned. 





Attachment 8: Dissolved Organic Carbon (DOC) Fractionation Sampling (Samples collected at selected sites)
Version 5 


Table 1.  DOC Fractionation Sampling Equipment
	
Item
	
Description Comments
	Manufacturer / Part #

	3x 1L amber glass pesticide bottles per sample
	Bottles purchased from the manufacturer have been pre-cleaned and combusted, and may be used without additional cleaning. 
	
USGS 1 stop shop Q27FLD

	Organic-grade water
	Distilled or nano-pure DI water
	USGS 1 stop shop N1580 or N1590



Filtration and Storage of Samples

1. Filtration for DOC Fractionation:  Please send 3-L of filtered sample.  The capsule filters currently used by the NASQAN program for nutrients are sufficient for DOC fractionation sample collection.  It is important to adhere to the NASQAN guidance that 2-L of DI water be pumped through the filter, plus enough native sample (~200-300mL) to saturate the filter before sample collection.  Therefore, collect the DOC fractionation sample after the rest of the NASQAN analytes from the capsule filter.  Fill three 1-L amber glass pesticides bottles with filtered water for DOC fractionation analysis.  If it is not possible to filter at least 2-L of sample (e.g. due to clogging of the filter), follow the high sediment sample guidelines outlined in item 2.

2. High sediment samples:  In the event that you encounter high sediment loads, please use the following for guidance:
a. If you are unable to collect at least 2-L of filtrate for DOC fractionation, you may use an additional filter.  Be sure to adhere to the NASQAN guidance and pass 2-L of DI water plus enough native water to saturate the second filter (~200-300mL) BEFORE collecting the DOC fractionation sample.
b. Note:  Please let Dave Reutter and Kenna Butler know when an additional filter was needed for DOC fractionation sample collection so that we can track filter costs.  

3. 
Equipment Blank:  Use standard NASQAN protocols for cleaning equipment used to collect and/or filter samples for DOC fractionation analysis.  Methanol and soap / detergent will contaminate these DOC samples. So, keep it away from equipment used for processing nutrient samples.  If the possibility of sufficient rinsing (or methanol or detergent is used) is a concern during the collection of any DOC fractionation sample, be sure to collect an equipment blank for DOC in a 125mL amber glass bottle (50-100mL) and send it along with your first couple of DOC fractionation samples for analysis.  This equipment blank can be collected in the laboratory.


Storing / Shipping Samples

Storage:  Once filtered, samples should be kept cold until shipment to the USGS NRP DOC laboratory in Boulder, CO, (George Aiken’s NRP project laboratory) either in a refrigerator (4-6ºC) or in a cooler with an adequate supply of ice. 

Shipping:  When possible, samples should be shipped immediately after collection/filtration.  If it is not feasible, use the storage guidance above and ship them as soon as possible.  Samples should always be shipped “priority overnight”.  The lab does NOT accept samples on Saturdays.  If samples are collected on Friday, please keep them cold over the weekend and ship them on Monday.  Similarly, if it can be avoided, we suggest not shipping samples on a Thursday before a long holiday weekend.

Care should be taken when shipping glass bottles.  
· Select a sturdy cooler with good handles.  
· Slip each amber glass bottle into an appropriately sized foam sleeve.  
· Glass bottles should never be laid on their side nor stacked for shipping.
· Standing the bottles up, pack them in the bottom of the cooler as tightly as possible, using packing materials (peanuts or bubble wrap) when necessary.  
· Use a large trash bag or several zip-lock bags to cover the top of the bottles with enough ice for shipping. 
· Fill the void space at the top of the cooler with packing materials.
· Ship the cooler priority overnight (FedEx) to:
	USGS
	Kenna Butler
	3215 Marine Street, STE E127
	Boulder, CO  80303
	Lab phone: 303-541-3057
	Kenna’s phone:  303-541-3009

· Important:  Include a completed return FedEx label to ensure the quick return of your cooler.


Labeling of Samples – Submission of ASRs

Please submit an ASR (NWQL form or equivalent is fine) with every sample that contain AT LEAST the following information:
· Site Name (and description when necessary)
· Sampling Date & Time
· USGS Site ID 
· Medium Code 
· Field pH
· Field Specific Conductance measurement (include units)

If you have any questions, please feel free to contact Kenna or George.


Contact Information:
Kenna Butler:  	Office = 303-541-3009
			Lab = 303-541-3057
			kebutler@usgs.gov	
George Aiken:	Office = 303-541-3036
			graiken@usgs.gov	

Vendors:
Fisher Scientific – 800-766-7000
USGS – http://1stop.usgs.gov/  























Attachment 9: DNA Sampling Protocol (Samples collected at selected sites)


Table 1.  DNA Sampling Equipment in each sample pack:

	Item
	Description
	Manufacturer/Part#

	Sterivex-GP Filter Unit with nipple outport

	Small, pre-sterilized 0.2-micron pore size filter capsule with luer lock adapter on in-port
	Fisher Sci/ SVGP01050


	1/4" hose-barb-to-male-luer-lock adaptor
	Used to attach Sterivex filter to peristaltic pump tubing
	Industrial Specialties CIML-14-300-PC

	10-ml syringe in sterile pack
	For pushing all liquid out of Sterivex filter unit after sample filtration
	

	Hemato-Seal capillary tube sealing putty in a small snap-cap tube
	For sealing outport of Sterivex filter.
	Fisher Sci/ 02-678

	1.5 ml DNA extraction/storage buffer in 3 ml syringe (“DEB”)
	For preserving DNA samples collected on Sterivex Filters
	See recipe below

	0.2 –micron syringe filter
	For pre-filtering DEB buffer
	Fisher Sci/ 09-719A

	Male luer plug (polycarbonate)
	For sealing inport of Sterivex filter.
	Ark-Plas/ AP117LMLP0CL



Table 2.  Storage and shipping equipment for each set of sample packs:

	Styrofoam shipping cooler

	Thick-walled Styrofoam cooler in a cardboard box for shipping
	various

	Ice packs
	Ice packs to be pre-frozen prior to shipping with samples
	various

	FedEx shipping label
	To be dated and attached to Styrofoam shipping cooler when samples are shipped
	FedEx




Filtration, Preservation, and Storage of Samples

Summary:  Water samples are pumped through Sterivex 0.2-micron pore size filter cartridges with a variable-speed pump fitted with a peristaltic pump head.  The best time to do this is immediately following sample collections using the USGS Capsule Filter currently used by the NASQAN program for nutrients.  The Sterivex filter is attached to the outflow end of the peristaltic pump tubing with a supplied hose-barb-to-male-luer-lock adapter.  (Note that luer-lock in-port will squeeze directly into some tubing without the adapter)

1. After completing sample collection with the USGS Capsule Filter:
a. Set up Sterivex filter:
i. Remove USGS Capsule Filter from the outflow end of the peristaltic pump tubing.
ii. Attach hose-barb-to-luer-lock adapter to the outflow end of the peristaltic pump tubing.
iii. Remove Sterivex filter cartridge from sterile pack and firmly attach to the male luer lock end of the adapter.
iv. (Alternative – skip step ii and squeeze in-port of sterivex into tubing.  This will work for some tubing)
b. Collect sample on Sterivex filter:
i. Make sure particles in the sample chamber are suspended evenly by continuing to churn sample (If Churn Splitter is used) or by whatever method was used for the USGS Capsule Filter sample collection.
ii. Pump sample slowly through Sterivex filter and direct the filtrate into a graduated cylinder or some other volumetric measuring device.  This is to measure the volume filtered.
iii. Stop filtering if one of these criteria is met:
1. Flow from outport of Sterivex filter slows from a stream to a drip.
2. ~250 ml of water is filtered.
3. If 250-ml of sample is not available, then stop when the allotted volume has been met.
c. Force all remaining water out of Sterivex Filter: 
i. Remove Sterivex filter from luer lock adapter.
ii. Remove 10-ml syringe from sterile pack, fill with air, attach to in-port of Sterivex filter
iii. Force remaining sample water out of Sterivex filter unit.  Repeat until there is only a small drop remaining.  It helps to shake/snap water out of the filter while holding pressure with the syringe.
d. Seal out-port of Sterivex filter:
i. Press nipple out-port into beige-colored hematocrit sealing putty supplied with sample kit in a small snap cap tube.
e. Add DNA extraction/preservation buffer:  Remove luer plug from 3-ml syringe labeled “DEB,” attach syringe to inport of 0.22 micron disk-shaped syringe filter, squeeze outport of syringe filter into inport of Sterivex filter.  Push buffer through syringe filter into Sterivex filter.  This should fill the Sterivex filter about half way (~1ml of DEB).
f. Seal in-port of Sterivex filter with Male Luer Plug
g. Label Sterivex filter with a sharpie marker to indicate:
i. Site Name
ii. Sampling date and time
iii. Volume filtered in mL
iv. USGS Site ID (when applicable)
h. Store Sterivex filter:
i. Put Sterivex filter and hose-barb-to-luer-lock adapter(s) in small ziplock bag included with sampling kit.  Throw away syringes, syringe filter, remaining hematocrit putty and packaging materials.
ii. Keep sample cold until it is returned to the lab.
iii. Once in the lab store Sterivex Filter in a freezer prior to shipping (-20ºC or -80ºC).

Labeling Samples
As described above, please label Sterivex filters with a Permanent Sharpie Marker, writing directly on the plastic housing of the filter unit to indicate:
1. Site Name
2. Sampling date and time
3. Volume filtered in mL
4. USGS Site ID (when applicable)

Shipping Samples
Samples should be accumulated in a freezer prior to shipping.  Store supplied ice packs in freezer as well.  When storage space becomes limiting, please pack samples and ice packs into the supplied Styrofoam cooler and ship to Byron Crump using the supplied FedEx label.  Please do not ship samples on a Friday because our laboratory is closed on Saturday and does not receive shipments.  Also, please email Byron Crump on the day the samples are shipped (bcrump@coas.oregonstate.edu).

Byron Crump
Associate Professor
College of Earth, Ocean, and Atmospheric Science
Oregon State University
104 CEOAS Admin Bldg
Corvallis, OR 97331-5503
Phone: 541-737-4369
Email: bcrump@coas.oregonstate.edu
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Attachment 10: Isotope Sampling Protocol (Samples collected at selected sites)

Field crews at all NASQAN stations should continue to collect aliquots from the composite water sample for analysis of stable isotopes of water. The 60-mL glass bottles for this sample are available from Ty Coplen. Email him at tbcoplen@usgs.gov to obtain the bottles. No filtering is required, but a filtered aliquot may be sent. Fill the 60-mL bottle 2/3 full of water and put on the Polyseal cap. No preservation is needed. Label the sample bottle with station id and the date and time of sample collection. Samples should be packaged securely and sent directly to Ty for analysis. Samples can be stored for 4 to 12 months before shipping so that multiple samples may be mailed together to reduce shipping and handling costs. Samples should be shipped to:

U.S. Geological Survey
Isotope Laboratory
431 National Center
12201 Sunrise Valley Dr
Reston, VA 20192

More information on collection of stable isotope samples is available at http://isotopes.usgs.gov/ and http://isotopes.usgs.gov/Instructions.htm#489.
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NASQAN DNA Sampling Protocol

SAMPLING KIT CONTENTS:

1 Sterivex capsule filters in sterile pack = [—_
1 metal hose-barb/luer-adapter (in plastic bag) m]
10-ml syringe in sterile pack [y — ]
1 small tube hematocrit putty (in plastic bag) @'

1 male luer plug (in plastic bag) .'

1 syringe containing DNA extraction buffer (DEB)
0.2-micron syringe prefilter -

1) Attach metal hose-barb/luer-adapter to "Sterivex" filter capsule. Attach to hose and pump

sample water through (250 ml or until filter is clogged).

Collect filtrate in graduated cylinder to P

estimate volume filtered.

2) Force remaining sample water out of filter capsule with air using 10 ml syringe. Shake

sample water out of the outport if necessary.
I—'—I = ]

3) Seal outport with hematocrit putty.

H—

4) Assemble buffer syringe. Remove luer plug on buffer syringe, and attach 0.2

micron prefilter to syringe.

5) Add approximately 1 ml buffer to filter cartridge through inport. Note that
0.5 ml of the 1.5 ml buffer contained in the DEB

DEB[J Eﬂ:l

syringe will remain in the prefilter. DEB:ﬂﬁ =

6) Seal in-port with male luer plug, label with sharpie, seal in ziplock bag.
Label should indicate Site Name, Date, Time, & Volume Filtered.

7) FREEZE = N [

Please return frozen samples and metal luer locks (they are expensive).
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1.5 ml DNA extraction buffer (Dé&)

After filtering sample: Seal outport with Assemble DEB syringe, Seal inport with
force out remaining putty prefilter, and sterivex. male luer plug
water with 10ml Add 1 ml DEB.
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